* PVP or silica coated particles with polar solves (water, ethanol)
  + Hydrophobic suspensions possible with dodecanethiol and polystyrene surfaces
* Drop-casting
  + Spreading a nanoparticle dispersion over a substrate and allowing it to try under controlled conditions
  + For small substrates (~1 cm^2)